- Documentazione ufficiale
- Guide della comunità
- 12.04 LTS

web wiki forum planet
help.ubuntu-it comunità italiana

- Desktop
- Server
- Ricerca

Questa guida non è stata ancora completamente tradotta. Se vuoi contribuire alla sua traduzione contatta il Gruppo Traduzione di Ubuntu-it.
Guida a Ubuntu Server » Rete »
Indietro | Avanti

# DHCP (Dynamic Host Configuration Protocol)

Il DHCP (Dynamic Host Configuration Protocol) è un servizio di rete che consente di assegnare automaticamente le impostazioni per agli host da un server, senza la necessità di dover configurare manualmente ogni singolo host nella rete. I computer configurati per essere client DHCP non hanno alcun controllo sulle impostazioni che ricevono dal server DHCP e la configurazione è trasparente all'utente del computer.

Le impostazioni comuni fornite da un server DHCP a un client includono:

- IP address and netmask

- IP address of the default-gateway to use

- IP adresses of the DNS servers to use

Un server DHCP può fornire anche altre proprietà di configurazione come:

- Nome dell'host

- Nome del dominio

- Server NTP (Network Time Protocol)

- Server di stampa

Il vantaggio di utilizzare DHCP è che i cambiamenti apportati alla rete, per esempio una modifica dell'indirizzo del server DNS, devono essere apportati solamente al server DHCP, mentre tutti gli host della rete vengono riconfigurati quando i client DHCP interrogano il server DHCP. Come ulteriore vantaggio, risulta anche molto semplice integrare nuovi computer nella rete, senza la necessità di controllare la disponibilità di un indirizzo IP. I conflitti nell'allocazione degli indirizzi IP sono quindi notevolmente ridotti.

A DHCP server can provide configuration settings using the following methods:

Manual allocation (MAC address)

  This method entails using DHCP to identify the unique hardware address of each network card connected to the network and then continually supplying a constant configuration each time the DHCP client makes a request to the DHCP server using that network device. This ensures that a particular address is assigned automatically to that network card, based on it's MAC address.

Dynamic allocation (address pool)

  In this method, the DHCP server will assign an IP address from a pool of addresses (sometimes also called a range or scope) for a period of time or lease, that is configured on the server or until the client informs the server that it doesn't need the address anymore. This way, the clients will be receiving their configuration properties dynamically and on a "first come, first served" basis. When a DHCP client is no longer on the network for a specified period, the configuration is expired and released back to the address pool for use by other DHCP Clients. This way, an address cand be leased or used for a period of time. After this period, the client has to renegociate the lease with the server to maintain use of the address.

Automatic allocation

  Using this method, the DHCP automatically assigns an IP address permanently to a device, selecting it from a pool of available addresses. Usually DHCP is used to assign a temporary address to a client, but a DHCP server can allow an infinite lease time.

The last two methods can be considered “automatic” because in each case the DHCP server assigns an address with no extra intervention needed. The only difference between them is in how long the IP address is leased, in other words whether a client's address varies over time. Ubuntu is shipped with both DHCP server and client. The server is dhcpd (dynamic host configuration protocol daemon). The client provided with Ubuntu is dhclient and should be installed on all computers required to be automatically configured. Both programs are easy to install and configure and will be automatically started at system boot.

- Installazione
- Configurazione
- Riferimenti

## Installazione

A un prompt di terminale, inserire il seguente comando per installare dhcpd:

    sudo apt-get install isc-dhcp-server

You will probably need to change the default configuration by editing /etc/dhcp/dhcpd.conf to suit your needs and particular configuration.

You also may need to edit /etc/default/isc-dhcp-server to specify the interfaces dhcpd should listen to.

I messaggi di dhcpd vengono inviati nel syslog, consultare quindi i relativi messaggi per quelli di diagnostica.

## Configurazione

Il messaggio di errore con cui si conclude l'installazione potrebbe essere fuorviante, ma i passi seguenti consentono di configurare il servizio.

Nella maggior parte dei casi si vuole assegnare un indirizzo IP in modo casuale. Questo può essere ottenuto con impostazioni come le seguenti:

    # minimal sample /etc/dhcp/dhcpd.conf
    default-lease-time 600;
    max-lease-time 7200;

    subnet 192.168.1.0 netmask 255.255.255.0 {
     range 192.168.1.150 192.168.1.200;
     option routers 192.168.1.254;
     option domain-name-servers 192.168.1.1, 192.168.1.2;
     option domain-name "mydomain.example";
    }

This will result in the DHCP server giving clients an IP address from the range 192.168.1.150-192.168.1.200. It will lease an IP address for 600 seconds if the client doesn't ask for a specific time frame. Otherwise the maximum (allowed) lease will be 7200 seconds. The server will also "advise" the client to use 192.168.1.254 as the default-gateway and 192.168.1.1 and 192.168.1.2 as its DNS servers.

After changing the config file you have to restart the dhcpd:

    sudo /etc/init.d/isc-dhcp-server restart

## Riferimenti

- The dhcp3-server Ubuntu Wiki page has more information.

- For more /etc/dhcp/dhcpd.conf options see the dhcpd.conf man page.

- ISC dhcp-server

Indietro | Avanti